Royva Dental Micromirrors for Magnification Work – RX-UT Series
“Crystal-clear image in a restricted operative field”
Royva RX-UT micromirrors are designed for precise microsurgical and endodontic procedures performed under a dental microscope. Their ultra-thin structure (0.7 mm thickness) combined with a 36-layer optical coating ensures exceptional sharpness and clarity of vision. The anti-reflective coating eliminates microscope light glare, providing safe and comfortable work even in hard-to-reach areas. An ergonomic metal alloy handle increases durability and ease of use.
Available models:
· RX-UT-Y03 – round, Ø 3 mm, single-sided
· RX-UT-Y05 – round, Ø 5 mm, single-sided
· RX-UT-F27 – rectangular, 2 × 7 mm, single-sided
· RX-UT-F39 – rectangular, 3 × 9 mm, single-sided
Key features:
· 36-layer optical coating for high resolution and image contrast
· Anti-reflective coating reducing microscope light glare
· Ultra-thin design – 0.7 mm thickness, weight 17 g
· Ergonomic, durable metal alloy handle
· Fully autoclavable, safe for repeated sterilization
Royva RX-UT Micromirrors USP:
· Ultra-thin and lightweight design ensuring maximum precision and comfort under the microscope
· Ultra-clear image thanks to advanced optical coatings, enhancing diagnosis and treatment efficiency
· Glare reduction providing excellent visibility of the operative field under intense illumination
· Variety of shapes and sizes to match individual clinical needs
	Black metal micromirrors:

	RX-UT-Y03
	Ultra-thin round micromirror 3 mm, 0.7 mm thickness, aluminum alloy handle, black, 1 pc

	RX-UT-Y05
	Ultra-thin round micromirror 5 mm, 0.7 mm thickness, aluminum alloy handle, black, 1 pc

	RX-UT-F27
	Ultra-thin rectangular micromirror 2 × 7 mm, 0.7 mm thickness, aluminum alloy handle, black, 1 pc

	RX-UT-F39
	Ultra-thin rectangular micromirror 3 × 9 mm, 0.7 mm thickness, aluminum alloy handle, black, 1 pc




Royva Ultra HD Mirror – Endodontic & Diagnostic Mirror with Endo Ruler
The Royva Ultra HD Mirror is an innovative dental mirror with a built-in endodontic ruler, combining superior image quality with functionality for precise root canal length measurement. Its 36-layer optical coating with >95.6% reflectivity delivers a sharp, natural image without glare. Thanks to its hydrophobic and anti-fog surface, the mirror remains clean and clear throughout the procedure. It is fully autoclavable and resistant to sterilization at 121°C (15 min) and 135°C (3.5 min). Available sizes: 22 mm (single-sided) and 24 mm (double-sided).
Key features:
· 36-layer optical coating ensuring high resolution and image clarity
· Integrated precision endodontic ruler for fast and accurate root canal measurements
· Hydrophobic surface (“lotus effect”) minimizing water and debris adhesion
· Anti-fog coating providing immediate resistance to fogging, even after sterilization
· Fully autoclavable with preserved durability and quality (15 min/121°C or 3.5 min/135°C)
· Optimal sizes and versions (22 mm single-sided, 24 mm double-sided) for various clinical applications
Royva Ultra HD Mirror USP:
· Endo-gauge function — precise canal length measurement without additional tools
· Ultra High Definition — >95.6% reflectivity, glare-free, natural color reproduction
· Hydrophobic and anti-fog — clear vision even in a moist oral environment
· High sterilization resistance — ensuring long-term durability and safety
· Clinical adaptability — two sizes and versions for optimal ergonomics
Endodontic ruler mirrors:
RS-Z-42H – Endo ruler mirror, single-sided, 22 mm, black, 5 pcs
RS-Z-42B – Endo ruler mirror, single-sided, 22 mm, blue, 5 pcs
RD-Z-52H – Endo ruler mirror, double-sided, 24 mm, black, 5 pcs
RD-Z-52B – Endo ruler mirror, double-sided, 24 mm, blue, 5 pcs
	Endodontic ruler mirrors:

	RS-Z-42H
	Endo ruler mirror, single-sided, 22 mm, black, 5 pcs

	RS-Z-42B
	Endo ruler mirror, single-sided, 22 mm, blue, 5 pcs

	RD-Z-52H
	Endo ruler mirror, double-sided, 24 mm, black, 5 pcs

	RD-Z-52B
	Endo ruler mirror, double-sided, 24 mm, blue, 5 pcs



